{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Формулы","Расчеты","Интервалы"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":57,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Формулы","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[[16,5,16,6],[13,0,13,1],[18,0,18,1],[16,0,16,1],[17,0,17,1],[11,0,11,1],[12,0,12,1],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[2,4,2,5],[3,4,3,5],[4,4,4,5],[5,4,5,5],[2,8,2,9],[3,8,3,9],[4,8,4,9],[5,8,5,9]],"flags":["formulas_cached_only"]}
[null,"Зависимость длинны и частоты (тона, ноты)"]
[]
["Скорость звука",null,344400,"мм\\с","Скорость звука",null,344400,"мм\\с"]
["Длинна",null,634,"мм","Частота",null,246.94,"Гц"]
["К",null,2.20031,null,"К",null,2.20031]
["Частота",null,246.8823327690834,"Гц","Длинна",null,633.8519436932004,"мм"]
[]
[]
[]
["Расчетные размеры (баланс)",{"$nulls":7},"УТАГУЧИ"]
[]
["Внутренний диаметр",null,21,"мм"]
["Длинна",null,656.3146145491581,"мм"]
["Диаметр отверстий",null,11.42287530066645,"мм"]
[]
[]
["Длинна",null,656,"мм",null,"Внутренний диаметр",null,21,"мм"]
["Внутренний диаметр",null,20.991610769487274,"мм",null,null,"Ширина",16.485,"мм"]
["Диаметр отверстий",null,11.419224521128227,"мм",null,null,"Глубина",3.2969999999999997,"мм"]
[]
[]
[]
["Комментарии:"]
[]
["1. Изменяемые (вносимые) параметры"]
["помечены зеленым цветом"]
[]
["2. Результаты расчетов помечены"]
["красным цветом"]

{"sheet":"Расчеты","index":1,"n_rows":26,"n_cols":15,"rows_kept":26,"cut":false,"hidden":false,"merged":[[14,12,14,13],[8,12,8,13],[9,12,9,13],[10,12,10,13],[11,12,11,13],[12,12,12,13],[13,12,13,13],[14,6,14,7],[8,9,8,10],[9,9,9,10],[10,9,10,10],[11,9,11,10],[12,9,12,10],[13,9,13,10],[14,9,14,10],[8,6,8,7],[9,6,9,7],[10,6,10,7],[11,6,11,7],[12,6,12,7],[13,6,13,7],[14,0,14,1],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[12,3,12,4],[13,3,13,4],[14,3,14,4],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[0,0,0,2],[1,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[0,5,0,6],[1,5,1,6],[2,5,2,6],[3,5,3,6],[4,5,4,6],[6,9,6,10],[7,9,7,10],[6,12,6,13],[7,12,7,13],[6,0,6,1],[7,0,7,1],[6,3,6,4],[7,3,7,4],[6,6,6,7],[7,6,7,7]],"flags":["formulas_cached_only"]}
["Длинна флейты",null,null,633.8519436932004,"мм","Базовая нота",null,246.93621524297154,"Гц"]
["Внутренний диаметр",null,null,21,"мм","EAR",null,29.432881713660034,null,"1--2",61.1993633034117,"мм- расcтояние между отверстиями"]
["Толщина стенки",null,null,5.4,"мм","BigNum",null,165674,null,"2--3",56.504200362505514,"мм"]
[{"$nulls":5},"TubeLength",null,670.9181957655987,null,"3--4",70.48405370110464,"мм- расcтояние между отверстиями"]
["Воспроизводимый диапазон",null,null,2.452740142805003,"октавы","MEL",null,30.7662520723984,null,"4--5",38.18877342014201,"мм- расcтояние между отверстиями"]
[]
["Te_1",null,12.9,"Te_2",null,12.9,"Te_3",null,12.525,"Te_4",null,12.9,"Te_5",null,12.9]
["Диаметр отверстия 1",null,10,"Диаметр отверстия 2",null,10,"Диаметр отверстия 3",null,9.5,"Диаметр отверстия 4",null,10,"Диаметр отверстия 5",null,10]
["Интервал1",null,3,"Интервал2",null,2,"Интервал3",null,2,"Интервал4",null,3,"Интервал5",null,2]
["LastLength1",null,670.9181957655987,"LastLength2",null,605.2525630926972,"LastLength3",null,543.3479956214765,"LastLength4",null,490.1790618588249,"LastLength5",null,418.1749812312381]
["Hz_1",null,293.6583041187851,"Hz_2",null,329.6203015442283,"Hz_3",null,369.9862788356877,"Hz_4",null,439.99031524478045,"Hz_5",null,493.872430485943]
["NewLength1",null,564.172705747782,"NewLength2",null,502.62074036046573,"NewLength3",null,447.7841732978872,"NewLength4",null,376.5401061335415,"NewLength5",null,335.45909788279937]
["S_1",null,53.372745008908396,"S_2",null,51.31591136611573,"S_3",null,47.781911161794625,"S_4",null,56.81947786264172,"S_5",null,41.357941674219376]
["CF_1",null,41.07985734491527,"CF_2",null,40.727255261010704,"CF_3",null,42.39488856093772,"CF_4",null,41.634875097696614,"CF_5",null,38.74264026709654]
["Отверстие 1",null,492.3265963304683,"Отверстие 2",null,431.1272330270566,"Отверстие 3",null,374.6230326645511,"Отверстие 4",null,304.13897896344645,"Отверстие 5",null,265.95020554330443]
[]
[]
["Как пользоваться калькулятором:"]
[]
["1. Все параметры помеченные зеленым цветом необходимо заполнить"]
["2. Красным помечены результаты расчетов"]
["3. Цифры для интервалов можно взять из таблицы во вкладке <Интервалы>."]
["Вы можете указать произвольный тераккорд главно, что бы сумма интервалов"]
["составляла 12!"]
["4. Расстояния до отверстий указаны от аккустического начала флейты,"]
["там где утагучи."]

{"sheet":"Интервалы","index":2,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":false,"merged":[[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4],[7,0,7,1],[8,0,8,1],[9,0,9,1],[6,0,6,1],[0,0,0,1],[0,3,0,4],[1,3,1,4],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,3,5,4],[1,0,1,1],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1]],"flags":["formulas_cached_only"]}
["Имя тетраккорда",null,"Интервалы","Ноты тетраккорда"]
["Минье",null,32232,"D F G A G D"]
["Мияко Буси",null,"14214","D Eb G A Bb D"]
["Рицу (земля)",null,"23223","D E G A B D"]
["Огонь",null,"33222","D F G# Bb C D"]
["Воздух",null,"32322","D F G Bb C D"]
["Вода",null,"23232","D E G A C D"]
["Облако",null,"22233","D E F# G# B D"]
["Рюкйю",null,"41241","D F# G A C# D"]